(1) Fixed the problem that anti-virus software would block the lighting software.
(2) Fixed the problem of incorrectly positioned points when importing .dxf files.
LedPlayer_K_v4.0:
(1) Support multi-color lamps such as 5 colors / 6 colors.
(2) The lighting function has been greatly improved.
LedPlayer-K V3.38.3:
(1) Fixed the problem that ghosting interface will be ghosted.
(2) Fixed the problem that the memory would increase when playing some video files.
(3) Added the function of writing code and writing parameters for SM17512, SM1752X, SM17500, UCS512F, TM512, GS8512.
LedPlayer-K V3.38.1:
(1) Optimized some functions of RDM.
LedPlayer-K V3.37.8:
(1) Fixed the ghosting issue of the RDM interface.
(2) Fix many problems of RDM.
LedPlayer-K V3.37.5:
(1) Added the function to modify the display model and ID number of T-600K-STD online.
LedPlayer-K V3.37.3:
(1) Optimized the RDMX software interface.
LedPlayer-K V3.37.2:
(1) RDMX can feedback the lamp status in real time.
LedPlayer-K V3.37:
(1) Added RDM function.
(2) Optimized DMX chip write parameter interface.
LedPlayer-K V3.36:
(1) Added the function of adjusting brightness regularly.
(2) Add test network status function.
(3) Optimized the problems when importing .DXF.
(4) Upgrade the built-in test effect to 256 gray level changes.
LedPlayer-K V3.35:
(1) The monitoring panel has been upgraded to monitor the status of each port.
(2) Added the function of writing code and writing parameters of SM17512.
(3) The write parameter function of UCS512CN has been upgraded.
(4) Modified the RGBW four-color separation mode.
(5) Fixed the problem when exporting XDAT.
LedPlayer-K V3.34:
(1) Built-in effects have been added to the online software.
(2) Upgraded the monitoring panel of the online software.
(3) When writing the address, you can write by channel or by number of lights.
(4) When writing addresses, the interval channel can start from 0.
(5) Added the function that peripheral devices can control this software through UDP or serial port.
(6) Modified the problem that the computer needs to be logged out or restarted after the software is forcibly closed.
(7) Added the function that the playback interface can change the playback frame rate.
LedPlayer-K V3.33.4:
(1) Add the function of writing code and writing parameters of UCS512D and UCS512E.
(2) Added the function of peripheral software to control this software.
LedPlayer-K V3.31:
(1) Added the function of controlling the play and pause of computers in the LAN.
LedPlayer-K V3.30:
(1) Added point-by-point correction function.
(2) Some other minor bugs have been modified.
LedPlayer-K V3.29:
(1) When setting T-500K for RGBW, set the position of W channel.
(2) When the text is input, a scale prompt for the position and speed of the text is added.
(3) The timing setting section has been revised.
(4) Added the function of playing pictures.
(5) Add UCS512C4 parameter writing function
(6) Fixed the bug that the picture in the invalid area remains when switching modes.
(7) Added split screen parameter copy function.
(8) Add the function of automatic startup after the computer is turned on for three minutes
(9) Restrict software to be opened only once.
(10) Increase APA102 and repair INK1003.
-------------------------------------------------- ------------------
LedPlayer-K V3.28:
(1) Importing DXF can magnify and solve the problem of errors.
(2) Adjust the canvas size to 0--19999
(3) Precision selection when importing DXF.
(4) Convert to MP4 after recording
(5) Fix the bug of input text length
(6) Prompt the total number of lights after importing dxf
(7) Added setting current function for UCS5603.
(8) TM1814 adds setting current function
(9) Support external control function to adjust brightness in real time